# The Function of Common Frequency Features

Feature extraction based on common frequency features.

## Description

Common frequency features are the statistical frequency features of the signal. "Data Upload" is used to load the required data set and label set, and the required features should be selected in the "Parameter" field.

## Parameter introduction

Parameters of common frequency features:

* Max: The largest value in the data. (data type: float)
* Min: The smallest value in the data. (data type: float)
* Mean: The result of dividing a sum of numbers by their number. (data type: float)
* Root Mean Square: The square root of the mean square (the arithmetic mean of the squares) of the data set. (data type: float)
* Standard Deviation: The square root of its variance. (data type: float)
* Variance: The expectation of the squared deviation of a random variable from its sample mean. (data type: float)
* Median: The central value. (data type: float)
* Skewness: A measure of the asymmetry of the probability distribution of a real-valued random variable about its mean. It is defined as (mean-median) / standard deviation. (data type: float)
* Kurtosis: The deviation of the curve of a distribution from the curve of a normal distribution. (data type: float)
* Peak to Peak Value: The difference between the highest and the lowest values in a waveform. (data type: float)
* Crest Factor: The peak amplitude of the waveform divided by the RMS value of the waveform. The crest factor indicates how extreme the peaks are in a waveform. (data type: float)
* Shape Factor: The ratio of the RMS value to the mean value of the signal. (data type: float)
* Impulse Factor: The ratio of peak value to mean value of the signal. (data type: float)

**Functional description of the main components**

The overall view of the function of common frequency features is divided into "Data Upload", and "Parameter".

图形用户界面, 应用程序

描述已自动生成

### Data Upload

The user needs to upload the data file and the label file. The uploaded data files support ".mat", ".txt", ".csv", ".xls", and ".npy" format files.

图形用户界面, 文本, 应用程序

描述已自动生成

### Parameter

The user can select the required features here.

图形用户界面, 文本, 应用程序

描述已自动生成

### Result

After the software has been run, click the "Download" button to download the relevant result data.

图形用户界面, 文本, 应用程序, 聊天或短信

描述已自动生成

**Examples**

The process of using common frequency features in feature extraction.

**Step 1: Configure the procedure**

Select "Feature Extraction and Reduction" from the process bar on the left side of the web page.



Then select the procedure that needs to be configured from the process display area.

图形用户界面, 文本, 应用程序, 聊天或短信

描述已自动生成

**Step 2: Upload the data file and the label file**

Select the data file and the label file to be applied from the local path.

图形用户界面, 文本, 应用程序

描述已自动生成

Click "Upload" after successfully selecting the upload data file, and then click "Save".

**Step 3: Select the function**

The ''Common Frequency Features'' function is chosen for feature extraction.

图形用户界面, 文本, 应用程序

描述已自动生成

**Step 4: Set and save the parameters**

**图形用户界面, 文本, 应用程序

描述已自动生成**

Firstly, the user needs to select features.

If the user clicks the "Select All" button, all common frequency features will be selected. Then if the user clicks the "Deselect All" button, all selected features are canceled.

Finally, click "Save" after the required features are selected.

**Step 5: Execute the configured procedure**

Before executing the configured function, the user also needs to set the selected output file format.

**图形用户界面, 文本, 应用程序, 聊天或短信

描述已自动生成**

Finally, select "Run".

**Step 6: Download**

When the progress bar reaches the end, the task is completed.

**图形用户界面, 文本

描述已自动生成**

Click "Download" to download the file of data.

